**Receiver Diagnostic / Sensor Data**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Variable** | **VR3-UWM** | **VMT** | **VR2W** | **VR2Tx** | **VR2AR** | **VR4-UWM** | **VR2C** | **HR2** |
| Temperature Samples (configurable interval) | - | - | - | (every 10 minutes to 24 hours, or not at all) | (every 10 minutes to 24 hours, or not at all) | (every 1 to 14 days) | (every 10 minutes to  60 hours, or not at all) | (every 1 minute to 24 hours) |
| Temperature Stats: Min, Max Average(configurable interval) | - | - | - | (every 10 minutes to 24 hours, or not at all) | (every 10 minutes to 24 hours, or not at all) | - | - | - |
| Ambient Noise Samples(configurable interval) | - | - | - | (every 10 minutes to 24 hours, or not at all) | (every 10 minutes to 24 hours, or not at all) | - | - | (every 1 minute to 24 hours) |
| Ambient Noise Stats: Min, Max Average(configurable interval) | - | - | - | (every 10 minutes to 24 hours, or not at all) | (every 10 minutes to 24 hours, or not at all) | - | - | - |
| Tilt Samples(configurable interval) | - | - | - | (every 10 minutes to 24 hours, or not at all) | (every 10 minutes to 24 hours, or not at all) | (every 1 to 14 days) | (every 10 minutes to 60 hours, or not at all) | (every 1 minute to 24 hours) |
| Tilt Stats: Min, Max, Average | - | - | - | - | - | - | - | - |
| Depth Samples(configurable interval) | - | - | - | - | (every 10 minutes to 24 hours, or not at all) | - | - | - |
| Depth Stats: Min, Max, Average(configurable interval) | - | - | - | - | (every 10 minutes to 24 hours, or not at all) | - | - | - |
| Detection Noise | - | - | - | - | - | - | - |  |
| Detection Signal Strength | - | - | - | - | - | - | - |  |
| Detection Quality Score | - | - | - | - | - | - | - |  |
| Ping Counts(not configurable) | (end of study) | (end of study) | (daily) | (daily) | (daily) | - | (daily) | (hourly) |
| Detection Counts(not configurable) | (end of study) | (end of study) | (daily) | (daily) | (daily) | - | (daily) | (hourly) |
| Ping Counts(configurable interval) | - | - | - | - | - | (every 1 to 14 days) | - | - |
| Detection Counts(configurable interval) | - | - | - | - | - | (every 1 to 14 days) | - | - |

If you have questions about any of this, please don’t hesitate to ask.

Cheers,

Stephanie